{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["例題31 非等温PBR"],"not_rendered":{"charts":1,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"例題31 非等温PBR","index":0,"n_rows":41,"n_cols":26,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
["微分方程式数",2,null,null,null,"Pt=",2.96,"MPa",null,null,null,null,"元問題条件",null,"化学工学会編：化学工学便覧 7版 p. 868",null,null,null,"L","V","触媒量W",null,0.02,870]
["V=","xA=","T=",null,null,"T0=",520,"°C",null,null,null,null,"L=",12,"m",null,null,null,"m","m3","kg",null,0.11,870]
[0.11000000000000006,0.80274225589104076,854.76863318664209,null,null,"FA0=",1.331,"mol/s","CH4",null,null,null,"R0=",5.3999999999999999E-2,"m","反応管半径",null,null,1,{"$f":"3.14*$N$3^2*S3","v":9.1562399999999995E-3},{"$f":"S3*3.14*$N$3^2*$N$5","v":10.987487999999999}]
[null,"xA'=","T'=",null,null,"FB0=",4.66,"mol/s","H2O",null,null,null,"a=",{"$f":"2/N3","v":37.037037037037038},"/m","(伝熱面積／反応器容積）",null,null,12,{"$f":"3.14*$N$3^2*S4","v":0.10987487999999999},{"$f":"S4*3.14*$N$3^2*$N$5","v":131.84985599999999}]
["微分方程式→",{"$f":"G12/G3","v":3.2028712364617107},{"$f":"(-G14*G15*(C3-G16)+(-G12)*(G17))/(G9*G13)","v":231.47171650621206},null,null,"FmolA",{"$f":"G3*(1-B3)","v":0.26255005740902476},"mol/s","CH4",null,null,null,"ρb=",1200,"kg/m3","触媒層密度(仮）"]
[null,null,null,null,null,"FmolB ",{"$f":"G4-G3*B3","v":3.5915500574090249},"mol/s","H2O",null,null,null,"k0=",110,"/s","例題31ではk0=11000とした",null,null,null,{"$f":"T4*210","v":23.073724799999997},92.3,"m3"]
["積分区間V=[a,",0,null,null,null,"FmolC",{"$f":"3*G3*B3","v":3.2053498277729258},"mol/s","H2 ",null,null,null,"R=",8.3140000000000002E-3,"kJ/mol-K=m3-kPa/mol-K"]
["b]",0.11,null,null,null,"FmolD",{"$f":"G3*B3","v":1.0684499425909753},"mol/s","CO",null,null,null,"E=",95.4,"kJ/mol ",null,null,null,null,null,"COCO計算結果"]
["積分刻み幅ΔV",5.0000000000000001E-3,null,null,null,"ΣFi=",{"$f":"SUM(G5:G8)","v":8.1278998851819502},"mol/s","全モル流量",null,null,null,"仮T=",520,"°C",null,null,null,null,null,"V[m3]","L[m]","FA","xA","V[m3]","T[°C]"]
["計算結果",null,null,null,null,"cA0=",{"$f":"(G3/(G3+G4))*G1/0.00000831/(G2+273.15)","v":99.773244370037418},"mol/m3",null,null,null,null,"xA",0,null,null,null,null,null,null,0,0,4.7880000000000003,{"$f":"1-W10/$W$10","v":0},0,520]
["V[m3]","xA","T[℃]",null,null,"cA=",{"$f":"(G5/G9)*G1/0.00000831/(C3+273.15)","v":10.201092556670948},"mol/m3",null,null,null,null,"仮cA",{"$f":"N21*(1-N10)","v":99.750216863627102},"mol/m3",null,null,null,null,null,1.0999999999999999E-2,{"$f":"U11/(3.14*$N$3^2)","v":1.2013664997859383},4.4000000000000004,8.1035923141186239E-2,{"$f":"Y12/2","v":5.4999999999999997E-3},749.5]
[0,0,520,null,"←初期値","(-rA')ρb",{"$f":"11000*G11*EXP(-1*95.4/0.00831/(C3+273.15))","v":4.263021615730537},"mol/m3-s",null,null,null,null,"(-rA')ρb",{"$f":"N6*EXP(-N8/N7/(N9+273.15))*N11","v":5.7187685264186326E-3},"mol/m3-s",null,null,null,null,null,2.1999999999999999E-2,{"$f":"U12/(3.14*$N$3^2)","v":2.4027329995718767},3.79,0.20843776106934009,1.0999999999999999E-2,796]
[5.0000000000000001E-3,3.546962196875697E-2,728.20529061462116,null,null,"Cp=",42,"J/mol-K",null,null,null,null,"ε=",0.432,null,null,null,null,null,null,3.3000000000000002E-2,3.6040994993578153,3.23,0.32539682539682546,2.1999999999999999E-2,812]
[0.01,8.9355444056466171E-2,786.31459501837162,null,null,"U=",1700,"J/m2-s-K","伝熱係数",null,null,null,"T0=",520,"℃","入口ガス温度",null,null,null,null,4.3999999999999997E-2,4.8054659991437534,2.76,0.4235588972431078,3.3000000000000002E-2,820]
[1.5000000000000001E-2,0.14831144914048783,806.33627635657592,null,null,"a=",37,"/m","(伝熱面積／反応器容積）",null,null,null,null,820,"℃","出口ガス温度",null,null,null,null,5.5E-2,6.0068324989296924,2.34,0.51127819548872189,4.3999999999999997E-2,826]
[0.02,0.20671234182448905,814.61336893982912,null,null,"Ta=",870,"°C","反応管外側温度",null,null,null,"P",2.96," MPa","入口圧力",null,null,null,null,6.6000000000000003E-2,7.2081989987156305,1.99,0.58437761069340022,5.5E-2,832]
[2.4999999999999998E-2,0.26236288330003421,819.28353058513721,null,null,"ΔrH=",206200,"J/mol","吸熱反応",null,null,null,null,2.6," MPa","出口圧力",null,null,null,null,7.6999999999999999E-2,8.4095654985015695,1.68,0.64912280701754388,6.6000000000000003E-2,837]
[2.9999999999999995E-2,0.31470058833598524,822.80901175592521,null,null,null,null,null,null,null,null,null,"Ta=",850,"℃","反応管外側温度",null,null,null,null,8.7999999999999995E-2,9.6109319982875068,1.41,0.70551378446115298,7.6999999999999999E-2,842]
[3.4999999999999996E-2,0.36371297771427613,825.89633805920278,null,null,null,null,null,null,null,null,null,"-ΔrH",-206.2,"kJ/mol",null,null,null,null,null,9.9000000000000005E-2,10.812298498073446,1.19,0.75146198830409361,8.7999999999999995E-2,846]
[0.04,0.40953810312340205,828.74595533802062,null,null,null,null,null,null,null,null,null,"U=",{"$f":"1/((1/83)+(1/14))","v":11.979381443298971},"J/(m2 s K)","伝熱係数",null,null,null,null,0.11,12.013664997859385,1,0.79114452798663326,9.9000000000000005E-2,849]
[4.5000000000000005E-2,0.45234655209845903,831.41837517366298,null,null,null,null,null,null,null,null,null,"cA0",{"$f":"N16*1000*O25/N7/(N14+273.15)","v":99.750216863627102},"mol/m3",null,null,null,null,null,null,null,null,null,0.11,852]
[5.000000000000001E-2,0.49231005257583899,833.93579166320171]
[5.5000000000000014E-2,0.52959387208742004,836.309605625166,null,null,null,null,null,null,null,null,null,"210本で",null,"反応管入口","出口"]
[6.0000000000000019E-2,0.56435538129906238,838.54788296417667,null,null,null,null,null,null,null,null,null,"ΣFmol","kmol/h",{"$f":"O29+O30","v":4529.2207792207791},{"$f":"SUM(P29:P32)","v":6622.727272727273}]
[6.5000000000000016E-2,0.59674412093770646,840.65743543601047,null,null,null,null,null,null,null,null,null,"A CH4","mole frac",{"$f":"O29/(O29+O30)","v":0.22222222222222224},{"$f":"P29/(SUM(P29:P32))","v":3.4954407294832825E-2}]
[7.0000000000000021E-2,0.62690218120288033,842.64444823135261,null,null,null,null,null,null,null,null,null,"B H2O","mole frac",{"$f":"O30/(O29+O30)","v":0.77777777777777779},{"$f":"P30/(SUM(P29:P32))","v":0.49696048632218842}]
[7.5000000000000025E-2,0.65496460205499507,844.51470239823709,null,null,null,null,null,null,null,null,null,"C H2","mole frac",null,{"$f":"P31/(SUM(P29:P32))","v":0.35106382978723405}]
[8.0000000000000029E-2,0.68105973179072943,846.27367564906751,null,null,null,null,null,null,null,null,null,"D CO","mole frac",null,{"$f":"P32/(SUM(P29:P32))","v":0.11702127659574468}]
[8.5000000000000034E-2,0.70530953816632846,847.92660056715681,null,null,null,null,null,null,null,null,null,"FmolA CH4","kmol/h",{"$f":"P32/P33","v":1006.4935064935065},{"$f":"O29*(1-P33)","v":231.49350649350649}]
[9.0000000000000038E-2,0.72782987921442521,849.47850362129361,null,null,null,null,null,null,null,null,null,"FmolB H2O","kmol/h",{"$f":"O29*3.5","v":3522.727272727273},{"$f":"O30-O29*(1-P33)","v":3291.2337662337663},"入口で(H2O)/(CH4)=3.5"]
[9.5000000000000043E-2,0.74873074267930206,850.93423286878988,null,null,null,null,null,null,null,null,null,"FmolC H2","kmol/h",null,{"$f":"3100*3/4","v":2325},"出口で水素とCOの合計量が3100"]
[0.10000000000000005,0.76811646210651696,852.29847768656725,null,null,null,null,null,null,null,null,null,"FmolD CO","kmol/h",null,{"$f":"3100/4","v":775}]
[0.10500000000000005,0.78608591622818913,853.57578241914291,null,null,null,null,null,null,null,null,null,"xA out",null,null,0.77,"反応管出口でのメタン反応率0.77"]
[0.11000000000000006,0.80273271692610138,854.77055528333267,null,null,null,null,null,null,null,null,null,"反応管1本あたり"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ΣFmol in","kmol/h",{"$f":"O24/210","v":21.567717996289424},{"$f":"P24/210","v":31.536796536796537}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"mol/s",{"$f":"O35*1000/3600","v":5.9910327767470628},{"$f":"P35*1000/3600","v":8.760221260221261}]
[null,null,null,null,null,null,null,null,null,null,null,null,"FmolA CH4","mol/s",{"$f":"O36*O25","v":1.3313406170549029},{"$f":"O37*(1-P41)","v":0.30620834192262764}]
[null,null,null,null,null,null,null,null,null,null,null,null,"FmolB H2O","mol/s",{"$f":"O36*O26","v":4.6596921596921597},{"$f":"O38-O37*(1-P41)","v":4.3534838177695319}]
[null,null,null,null,null,null,null,null,null,null,null,null,"FmolC H2","mol/s",null,{"$f":"3*O37*P41","v":3.0753968253968256}]
[null,null,null,null,null,null,null,null,null,null,null,null,"FmolD CO","mol/s",null,{"$f":"O37*P41","v":1.0251322751322753}]
[null,null,null,null,null,null,null,null,null,null,null,null,"xA out",null,null,0.77]