{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["例題23a SO2水吸収","COCO_23a結果整理","SO2水平衡"],"not_rendered":{"charts":6,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"例題23a SO2水吸収","index":0,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["微分方程式数",2,null,null,null,"定数",null,null,null,null,"元例題"]
["z=","y=","x=",null,null,"m=",30,null,null,null,"疋田　化学工学通論 p. 168 例題6.4"]
[3.4999999999999956,6.3888767435209895E-3,-8.0569461322601031E-5,null,null,"kya=",125,"mol/m3-s",null,null,"伊東　ベーシック分離工学　p.71 例題3.8"]
[null,"y'=","x'=",null,null,"kxa=",7003,"mol/m3-s",null,null,"Henley, Seader, Roper: Separation Process Principles p. 255 Example 6.10"]
["微分方程式→",{"$f":"-(G3/G6)*(B3-G2*(G5*C3-B3)/(G5-G2))","v":-1.1469941777019016E-2},{"$f":"-(G4/G13)*((G5*C3-B3)/(G5-G2)-C3)","v":-2.5591124000488651E-4},null,null,"D=",{"$f":"-G4/G3","v":-56.024000000000001},null,null,null,null,null,"疋田　化学工学通論 p. 168 例題6.4"]
[null,null,null,null,null,"G=",62.5,"mol/m2-s",null,null,null,null,"HG",0.5,"m"]
["積分区間z=[a,",0,null,null,null,"yB=",0.1,null,null,null,null,null,"kya=G/HG",{"$f":"G6/N6","v":125}]
["b]",3.5,null,null,null,"xB*=",{"$f":"G7/G2","v":3.3333333333333335E-3},null,null,null,null,null,"HL",0.4,"m"]
["積分刻み幅Δz",0.1,null,null,null,"yT=",0.01,null,null,null,null,null,"kxa=L/HL",{"$f":"G13/N8","v":7003.1250000000009}]
["計算結果",null,null,null,null,"xT=",0]
["z [m]","y","x","yi","xi","Lmin=",{"$f":"G6*(G7-G9)/(G8-G10)","v":1687.5000000000002},"mol/m2-s"]
[0,{"$f":"G7","v":0.1},{"$f":"G14","v":2.008032128514056E-3},{"$f":"$G$2*($G$5*C12-B12)/($G$5-$G$2)","v":7.4106525609552512E-2},{"$f":"($G$5*C12-B12)/($G$5-$G$2)","v":2.4702175203184171E-3},"CL=",1.66]
[0.1,9.49312409501685E-2,1.8949406726945224E-3,{"$f":"$G$2*($G$5*C13-B13)/($G$5-$G$2)","v":7.012928852315857E-2},{"$f":"($G$5*C13-B13)/($G$5-$G$2)","v":2.3376429507719521E-3},"L=",{"$f":"G12*G11","v":2801.2500000000005},"mol/m2-s"]
[0.2,9.007615202226954E-2,1.7866165109832561E-3,6.6319709185900036E-2,2.2106569728633342E-3,"xB=",{"$f":"(G6/G13)*(G7-G9)+G10","v":2.008032128514056E-3}]
[0.3,8.5425726096304361E-2,1.6828586813097805E-3,6.2670720098345858E-2,2.0890240032781955E-3]
[0.39999999999999997,8.0971335741347877E-2,1.5834746930242722E-3,5.917555168674081E-2,1.9725183895580268E-3]
[0.49999999999999994,7.670471721001168E-2,1.4882801697905328E-3,5.5827719744149254E-2,1.8609239914716418E-3]
[0.6,7.26179551076096E-2,1.3970985075325659E-3,5.2621013401009289E-2,1.7540337800336428E-3]
[0.70000000000000007,6.8703467707584343E-2,1.3097605468001864E-3,4.9549483602779915E-2,1.6516494534259971E-3]
[0.80000000000000016,6.4953992885952327E-2,1.2261042589458355E-3,4.6607432073305297E-2,1.5535810691101764E-3]
[0.90000000000000024,6.1362574648672605E-2,1.1459744455304022E-3,4.3789400743420852E-2,1.4596466914473618E-3]
[1.0000000000000002,5.7922550226945389E-2,1.0692224504003885E-3,4.1090161625189511E-2,1.3696720541729838E-3]
[1.1000000000000003,5.4627537716499655E-2,9.9570588390226859E-4,3.8504707112982546E-2,1.2834902370994182E-3]
[1.2000000000000004,5.1471424237938185E-2,9.2528835872240532E-4,3.6028240693411914E-2,1.2009413564470638E-3]
[1.3000000000000005,4.8448354596175303E-2,8.5783923686245705E-4,3.3656168046879105E-2,1.1218722682293035E-3]
[1.4000000000000006,4.5552720417928391E-2,7.9323338728086597E-4,3.1384088524232176E-2,1.0461362841410727E-3]
[1.5000000000000007,4.2779149747111098E-2,7.3135095375080584E-4,2.9207786982718628E-2,9.7359289942395427E-4]
[1.6000000000000008,4.0122497078825752E-2,6.7207713250392177E-4,2.7123225966088117E-2,9.0410753220293723E-4]
[1.7000000000000008,3.7577833813466119E-2,6.1530195924734818E-4,2.5126538214337701E-2,8.3755127381125683E-4]
[1.8000000000000009,3.5140439113221004E-2,5.6092010515888064E-4,2.321401948920376E-2,7.7380064964012527E-4]
[1.900000000000001,3.2805791144015793E-2,5.0883068148183444E-4,{"$f":"$G$2*($G$5*C31-B31)/($G$5-$G$2)","v":2.1382121702090376E-2},{"$f":"($G$5*C31-B31)/($G$5-$G$2)","v":7.1273739006967921E-4}]
[2.0000000000000009,3.0569558686644037E-2,4.5893705235707422E-4,{"$f":"$G$2*($G$5*C32-B32)/($G$5-$G$2)","v":1.9627446331685377E-2},{"$f":"($G$5*C32-B32)/($G$5-$G$2)","v":6.5424821105617922E-4}]
[2.1000000000000005,2.8427593101526157E-2,4.1114665554498406E-4,{"$f":"$G$2*($G$5*C33-B33)/($G$5-$G$2)","v":1.7946738119052244E-2},{"$f":"($G$5*C33-B33)/($G$5-$G$2)","v":5.9822460396840812E-4}]
[2.2000000000000002,2.6375920632188292E-2,3.6537083070478177E-4,{"$f":"$G$2*($G$5*C34-B34)/($G$5-$G$2)","v":1.6336879028501228E-2},{"$f":"($G$5*C34-B34)/($G$5-$G$2)","v":5.4456263428337426E-4}]
[2.2999999999999998,2.4410735033182848E-2,3.2152465491260316E-4,1.4794882463035848E-2,4.9316274876786163E-4]
[2.3999999999999995,2.2528390508774056E-2,2.7952678511321028E-4,1.3317887723643361E-2,4.4392959078811203E-4]
[2.4999999999999991,2.0725394949288514E-2,2.3929930721304201E-4,1.1903154702150089E-2,3.9677182340500301E-4]
[2.5999999999999988,1.8998403452582777E-2,2.007675915346454E-4,1.0548058797795877E-2,3.5160195992652921E-4]
[2.6999999999999984,1.7344212118609148E-2,1.6386015436432795E-4,9.2500860480969008E-3,3.0833620160323002E-4]
[2.799999999999998,1.5759752105567345E-2,1.2850852533617527E-4,8.0068284649636948E-3,2.6689428216545647E-4]
[2.8999999999999977,1.4242083936615099E-2,9.4647120406406298E-5,6.8159795674219764E-3,2.2719931891406587E-4]
[2.9999999999999973,1.2788392046575527E-2,6.2213120182408725E-5,{"$f":"$G$2*($G$5*C42-B42)/($G$5-$G$2)","v":5.6753301026486085E-3},{"$f":"($G$5*C42-B42)/($G$5-$G$2)","v":1.8917767008828692E-4}]
[3.099999999999997,1.1395979558524382E-2,3.114635338073213E-5,4.5827639473843985E-3,1.5275879824614664E-4]
[3.1999999999999966,1.0062263280566745E-2,1.389185197830812E-6,3.5362541821201128E-3,1.1787513940400375E-4]

{"sheet":"COCO_23a結果整理","index":1,"n_rows":30,"n_cols":20,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
["<COCO_23a_AbsorpSO2.fsd>計算結果",null,null,null,null,null,null,null,null,0.1,2.0551200000000001E-3]
["mole fraction",null,null,null,null,null,null,null,null,6.3936699999999999E-2,2.0551200000000001E-3]
["Stage","x","y","操作線x","y",null,null,null,null,6.3936699999999999E-2,1.23657E-3]
["feed",0,null,null,null,null,null,null,null,3.85741E-2,1.23657E-3]
[1,2.6075000000000002E-4,8.0269599999999997E-3,0,8.0269599999999997E-3,null,null,null,null,3.85741E-2,6.5786000000000002E-4]
[2,6.5786000000000002E-4,2.0364400000000001E-2,2.6075000000000002E-4,2.0364400000000001E-2,null,null,null,null,2.0364400000000001E-2,6.5786000000000002E-4]
[3,1.23657E-3,3.85741E-2,6.5786000000000002E-4,3.85741E-2,null,null,null,null,2.0364400000000001E-2,2.6075000000000002E-4]
[4,2.0551200000000001E-3,6.3936699999999999E-2,1.23657E-3,6.3936699999999999E-2,null,null,null,null,8.0269599999999997E-3,2.6075000000000002E-4]
["feed",null,0.1,2.0551200000000001E-3,0.1,null,null,null,null,8.0269599999999997E-3,0]
[]
[]
[]
[]
["段","x","段","y"]
[0.5,0,0.5,8.0269599999999997E-3]
[1.5,2.6075000000000002E-4,1.5,2.0364400000000001E-2]
[2.5,6.5786000000000002E-4,2.5,3.85741E-2]
[3.5,1.23657E-3,3.5,6.3936699999999999E-2,null,null,null,null,null,null,null,null,null,null," "]
[4.5,2.0551200000000001E-3,4.5,0.1,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]

{"sheet":"SO2水平衡","index":2,"n_rows":13,"n_cols":18,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["SO2の水に対する溶解度",null,null,null,"20℃",null,null,null,null,null,null,null,null,null,null,"m=",30]
["疋田 p. 163",null,null,"COCO EOS/Predictive SRK"]
["x","y",null,"x","y",null,null,null,null,null,null,null,null,null,null,null,0,0]
[0,0,null,6.0999999999999999E-5,1.89E-3,null,null,null,null,null,null,null,null,null,null,null,3.0000000000000001E-3,{"$f":"Q4*Q1","v":0.09}]
[1.4100000000000001E-4,1.58E-3,null,1.2300000000000001E-4,3.7699999999999999E-3]
[2.81E-4,4.2199999999999998E-3,null,3.0600000000000001E-4,9.3799999999999994E-3]
[5.62E-4,1.12E-2,null,6.0769999999999997E-4,1.8589999999999999E-2]
[8.43E-4,1.8599999999999998E-2,null,1.196E-3,3.653E-2]
[1.41E-3,3.44E-2,null,1.7600000000000001E-3,5.3800000000000001E-2]
[1.9599999999999999E-3,5.1299999999999998E-2,null,2.8500000000000001E-3,8.6699999999999999E-2]
[2.81E-3,7.7600000000000002E-2,null,4.3699999999999998E-3,0.13200000000000001]
[4.1999999999999997E-3,0.12]
[6.9800000000000001E-3,0.21199999999999999]