{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["例題29非等温CSTR","fogler_ex_11_3"],"not_rendered":{"charts":5,"images":3,"macros":1,"external_links":0,"defined_names":27,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"例題29非等温CSTR","index":0,"n_rows":10,"n_cols":6,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["反応率 xA",0.4097334724050164,null,"反応器容積V",1.2,"m3"]
["反応温度T",345.26240649921061,"K","供給温度T0",330,"K"]
["CSTR設計方程式(1)",{"$f":"E5*B1-E1*E10","v":-4.2134438248886852E-2},null,"全供給　F",163,"kmol/h"]
["熱収支(2)",{"$f":"(E3*E6*(E2-B2)+(-E7)*B1*E5)/1000","v":3.2877135329064916E-2},null,"供給濃度cA0",9.3000000000000007,"kmol/m3"]
[null,{"$f":"SUMSQ(B3:B4)","v":2.8562169139949075E-3},null,"供給反応物 FA0",146.69999999999999,"kmol/h"]
[null,null,null,"熱容量　Cp",166.7,"kJ/kmol-K"]
[null,null,null,"反応熱　ΔrH",-6900,"kJ/kmol "]
[null,null,null,"k",{"$f":"31.1*EXP((65700/8.31)*((1/360)-(1/B2)))","v":12.17978025436679},"/h"]
[null,null,null,"Kc",{"$f":"3.03*EXP((-6900/8.31)*((1/333)-(1/B2)))","v":2.7732061897978193}]
[null,null,null,"-rA",{"$f":"E8*E4*(1-(1+(1/E9))*B1)","v":50.125029033387328},"kmol/m3-h"]

{"sheet":"fogler_ex_11_3","index":1,"n_rows":52,"n_cols":14,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
["微分方程式数",1,null,null,null,"定数"]
["V=","X=",null,null,null,"FA0=",146.69999999999999,"kmol/h","n-butane"]
[0,0,null,null,null,"CA0=",9.3000000000000007,"kmol/m3","n-butane"]
[null,"X'=",null,null,null,"CA ",{"$f":"G3*(1-B3)","v":9.3000000000000007},null,"n-butane"]
["微分方程式→",{"$f":"G9/G2","v":0.26776859786073121},null,null,null,"CB",{"$f":"G3-G4","v":0},null,"isobutane"]
[null,null,null,null,null,"T",{"$f":"330+43.3*B3","v":330},"K"]
["積分区間W=[a,",0,null,null,null,"k",{"$f":"31.1*EXP(7906*(G6-360)/(360*G6))","v":4.2238336888354047},"/h","31.1*EXP(7906*(T-360)/(360*T))"]
["b]",5,null,null,null,"Kc",{"$f":"3.03*EXP((-6900/8.31)*(1/333-1/G6))","v":3.0994680879150969},null,"3.03*EXP((-6900/8.31)*(1/333-1/T))"]
["積分刻み幅ΔW",0.25,null,null,null,"-rA",{"$f":"G7*(G4-G5/G8)","v":39.281653306169268}]
["計算結果",null,null,null,null,null,null,null,null,null,null,"n-butane","isobutane"]
["V[m3]","X",null,null,"CA[kmol/m3]","CB","T","k","Kc","-rA[kmol/h m3]","F[kmol/h]","FA[kmol/h]","FB[kmol/h]","(FA0/-ra)"]
[0,0,null,null,{"$f":"$G$3*(1-B12)","v":9.3000000000000007},{"$f":"$G$3-E12","v":0},{"$f":"330+43.3*B12","v":330},{"$f":"31.1*EXP(7906*(G12-360)/(360*G12))","v":4.2238336888354047},{"$f":"3.03*EXP((-6900/8.31)*(1/333-1/G12))","v":3.0994680879150969},{"$f":"H12*(E12-F12/I12)","v":39.281653306169268},163,{"$f":"G2","v":146.69999999999999},{"$f":"$L$12*B12","v":0},{"$f":"$G$2/J12","v":3.7345678619122795}]
[0.25,7.1207181043231038E-2,null,null,{"$f":"$G$3*(1-B13)","v":8.6377732162979513},{"$f":"$G$3-E13","v":0.66222678370204946},{"$f":"330+43.3*B13","v":333.08327093917188},{"$f":"31.1*EXP(7906*(G13-360)/(360*G13))","v":5.2725421763465397},{"$f":"3.03*EXP((-6900/8.31)*(1/333-1/G13))","v":3.028111783673848},{"$f":"H13*(E13-F13/I13)","v":44.389955642448079},163,{"$f":"$L$12*(1-B13)","v":136.25390654095798},{"$f":"$L$12*B13","v":10.446093459041993},{"$f":"$G$2/J13","v":3.3048016803990112}]
[0.5,0.15156211120855634,null,null,7.8904723657604263,1.4095276342395744,336.56263941533047,6.7388700561112094,2.9510715476580938,49.954164708869229,163,{"$f":"$L$12*(1-B14)","v":124.46583828570478},22.234161714295212,2.9366920827314682]
[0.75,0.24134767837776144,null,null,7.0554665910868186,2.2445334089131821,340.45035447375705,8.8122007057312128,2.8690931632988419,55.280274591893736,163,111.29429558198238,35.405704418017599,2.6537494808593438]
[1,0.33894629755198441,null,null,6.1477994327665462,3.1522005672334545,344.6763746840009,11.71488841629785,2.7845688184172324,58.759241795524808,163,96.976578149123881,49.723421850876107,2.4966285390560108]
[1.25,0.4390478564736961,null,null,5.2168549347946263,4.0831450652053745,349.01077218531105,15.575871111508699,2.7024951040400595,57.723792177934797,163,82.291679455308767,64.408320544691207,2.5414130718888699]
[1.5,0.53172844186311186,null,null,4.3549254906730601,4.9450745093269406,353.02384153267275,20.150536682956069,2.6303864587286361,49.871475495945631,163,68.695437578681492,78.004562421318496,2.9415612540263854]
[1.75,0.60573679396454239,null,null,3.666647816129756,5.6333521838702447,356.22840317866468,24.64792681221909,2.5753161798158803,36.459381495535276,163,57.838412325401627,88.861587674598354,4.0236557501109695]
[2,0.65565645525841276,null,null,3.2023949660967617,6.097605033903239,358.38992451268928,28.178153841714629,2.5393656962816884,22.57530591340883,163,50.51519801359084,96.184801986409141,6.4982508127549252]
[2.25,0.68467459478395443,null,null,2.9325262685092239,6.3674737314907768,359.64640995414521,30.435708117045252,2.5188945195714019,12.315566994889302,163,46.258236945193879,100.4417630548061,11.911753641620995]
[2.5,0.69988601506264603,null,null,2.7910600599173923,6.5089399400826089,360.30506445221255,31.683686775026821,2.5082860319043467,6.212692637252875,163,44.026721590309826,102.67327840969017,23.612949902003798]
[2.75,0.70739407002783694,null,null,2.7212351487411168,6.5787648512588834,360.63016323220535,32.316649057377788,2.5030805970413366,3.0044097443220283,163,42.925289926916321,103.77471007308367,48.828226668231679]
[3,0.71098526135130802,null,null,2.6878370694328355,6.6121629305671652,360.78566181651161,32.623446423938773,2.500597906700154,1.422522512346857,163,42.398462159763113,104.30153784023688,103.12666318227643]
[3.25,0.71267662160207712,null,null,2.6721074191006831,6.6278925808993172,360.85889771536995,32.768855009258786,2.4994302159531512,0.66671558943875175,163,42.15033961097528,104.54966038902471,220.03385300093794]
[3.5,0.71346735192814947,null,null,2.66475362706821,6.6352463729317908,360.89313633848889,32.837037011975802,2.4988846566929706,0.31098174606650864,163,42.034339472140466,104.66566052785952,471.73186804548249]
[3.75,0.71383574582393328,null,null,2.6613275638374208,6.6386724361625795,360.90908779417629,32.868846371179337,2.4986305617173059,0.14472783457605368,163,41.980296087628986,104.719703912371,1013.626718244789]
[4,0.71400709879542335,null,null,2.6597339812025629,6.6402660187974378,360.91650737784181,32.883651562906458,2.4985123896543704,6.72842952806504E-2,163,41.955158606711393,104.7448413932886,2180.3007579717928]
[4.25,0.71408674086826407,null,null,2.6589933099251444,6.6410066900748568,360.91995587959582,32.890534837689586,2.4984574687587737,3.1265358247543229E-2,163,41.943475114625656,104.75652488537433,4692.0940050807631]
[4.5,0.71412374419584346,null,null,2.6586491789786559,6.6413508210213443,360.92155812368003,32.893733392665339,2.4984319521610061,1.4524948107661901E-2,163,41.938046726469764,104.76195327353022,10099.863965959081]
[4.75,0.71414093388572286,null,null,2.6584893148627775,6.6415106851372236,360.9223024372518,32.895219359726418,2.4984200987332446,6.7471441974047966E-3,163,41.935524998964453,104.76447500103554,21742.53220442899]
[5,0.71414891865427355,null,null,2.6584150565152562,6.6415849434847445,360.92264817773003,32.895909625798161,2.4984145927431305,3.1340370600823134E-3,163,41.93435363341807,104.76564636658192,46808.636014070304]
[]
[]
[]
[]
["COCO <Fogler_11_3.fsd>"]
["V",{"$f":"11*(3.14/4)*0.7^2","v":4.2311499999999995},"m3"]
[]
[null,"V","temperature",null,"FA","X",null,"V","rxn1 rate profile"]
["section","m3","℃","K","kmol/h",null,null,null,"kmol/m3-h"]
[0,{"$f":"$B$38*A42/100","v":0},56.85,{"$f":"C42+273.15","v":330},146.69999999999999,{"$f":"($E$42-E42)/$E$42","v":0},0,{"$f":"$B$38*G42/100","v":0},34.4]
[20,{"$f":"$B$38*A43/100","v":0.84622999999999993},66.819999999999993,{"$f":"C43+273.15","v":339.96999999999997},112.5,{"$f":"($E$42-E43)/$E$42","v":0.23312883435582815},10,{"$f":"$B$38*G43/100","v":0.42311499999999996},40.46]
[40,1.6924599999999999,77.8,350.95,73.3,0.5003408316291752,20,0.84622999999999993,45.99]
[60,2.5386899999999999,84.17,357.32,49.5,0.66257668711656437,30,1.2693449999999999,47.7]
[80,3.3849199999999997,85.86,359.01,43,0.70688479890933875,40,1.6924599999999999,41.36]
[100,{"$f":"$B$38*A47/100","v":4.2311499999999995},86.16,359.30999999999995,41.86,0.71465576005453302,50,2.1155749999999998,28.02]
[null,null,null,null,null,null,60,2.5386899999999999,15.05]
[null,null,null,null,null,null,70,2.9618049999999996,6.94]
[null,null,null,null,null,null,80,3.3849199999999997,2.96]
[null,null,null,null,null,null,90,3.8080349999999998,1.21]
[null,null,null,null,null,null,100,4.2311499999999995,0.49]